Confined Space Entry Permit
Permit-Required Confined Space (29 CFR 1910.146) — Valid for one shift only — safetyteamtech.com
Entry Details
	Field
	Entry

	Space identification / location
	

	Purpose of entry
	

	Date
	

	Authorized time period (this shift only)
	From: __________ To: __________

	Authorized entrants (names)
	

	Attendant (name)
	

	Entry supervisor (name, signature)
	


Hazard Identification & Isolation
	Field
	Entry

	Hazards identified
	[ ] Atmospheric   [ ] Engulfment   [ ] Entrapment   [ ] Other: __________

	Isolation methods completed
	[ ] Lockout/Tagout   [ ] Blanking   [ ] Disconnection   [ ] N/A


Atmospheric Testing (record actual readings, not just “OK”)
	Field
	Entry

	Oxygen level (acceptable: 19.5%–23.5%)
	

	Flammability / LEL reading (acceptable: below 10%)
	

	Toxic gas reading(s)
	

	Time of testing / tester’s initials
	


Rescue, Communication & Equipment
	Field
	Entry

	Rescue / emergency service and how to summon
	

	Communication method (attendant ↔ entrants)
	

	Required equipment (PPE, monitor, comms, retrieval)
	

	Additional permits required (e.g. hot work)
	


Permit Closeout
	Field
	Entry

	Permit canceled / entry complete (time)
	

	Entry supervisor signature
	



This permit is valid for the specific task and shift described above only. Post at the entry point for the duration of the work. If conditions change or work extends beyond the authorized period, cancel this permit and complete a new one before re-entry. Free template provided by Safety Team Technologies (safetyteamtech.com). Not a substitute for your own OSHA 1910.146 program review.
